Operation Instruction for the

Pressure Test Platform

First, please Select DN50 pipe section and fix it on the stainless steel bracket (tighten the bolts), and install the test meter DN50 and clamp it.

Second, Open the main interface screen, modify the set parameters according to the automatic parameters. Set the pressure as it is required, and set the evacuation time (usually 20 seconds). Pressure holding time is set according to company technical requirements.

Third, Press the Main Interface button to select Automatic.

Fourth, Press the start key to start the platform automatically.

Fifth, Check whether the meter is leaking; if it is not leaking, the meter is qualified; if it is leaking, the meter should be disqualified.

At last, Unload the meter, the batch is tested. You can continue to the next batch.